         Welcome to LegaSuite License and Message Server

1 Installing the LegaSuite License and Message Server on the IBM i

This file only contains instructions for installing the License
and Message Server (LMS). Additional instructions for using this
product can be found in the Client or Server on-line help.


IMPORTANT
=========
LegaSuite IBM i products have the option to be automatically
installed to your IBM i when using TCP/IP (required).
If you choose to use this feature, simply start the automatic
install procedure and follow the provided instructions.

Before installing the LegaSuite License and Message Server, please
ensure that there is no version of LegaSuite License and Message
Server running on your IBM i.

This installation will save and restore any licenses from LegaSuite
products previously present on your IBM i. If you are upgrading
from GUI/400 License Manager and TCP/IP and/or SPX/IPX used for
connection to License Manager, adapt your SERVICES files on both
IBM i and pc.
See section 1.1.3 and 1.1.4 in this README.

1.1 Before installing
Before installing the LegaSuite License and Message Server, you
should check the following points.

1.1.1 OS/400
This installation covers V6R1 and higher installation.

1.1.2 Connecting Client/Server to License and Message Server (LMS) over TCP/IP.
Both Client/Server and LMS daemon need to know which PORT to
use for the connection. They both have a default value of 1025.
If this value conflicts with another TCP/IP application, then
this default port can be changed as follows.

1.1.3 On the IBM i
     - Use WRKSRVTBLE to add a table entry for service 'sealms'
       using protocol 'tcp'. It is advisable to do this even if the
       default port is used. This allows WRKTCPSTS to give the port
       name.
       It also ensures that when another service is installed, it
       can be seen in the services file that this port is already
       in use.
     - It is also possible to specify another PORT when starting the
       LMS daemon by specifying PORT(xxxx) at STRLMSTCP command.

     Determining PORT to be used:
     a) If PORT(xxxx) specified at STRLMSTCP, use port 'xxxx',
     b) else if PORT(*DFT), look for 'sealms' entry in SERVICES file
     c) else use default port 1025.


1.1.4 On the PC
     - Add an entry to the SERVICES file for protocol 'sealms'
       using protocol 'tcp'. It is advisable to do this even if the
       default port is used. This makes centralized maintenance
       possible.
     - It is also possible to specify another PORT in the used
       section of Client/Server's INI file, or on the command line
       using the parameter 'TcpIpLicensePort='.

     Determination PORT to be used:
     a) If parameter '/GTcpIpLicensePort=xxxx' specified on
        commandline, use port 'xxxx',
     b) else if 'TcpIpLicensePort=yyyy' is specified in used
        section of INI file, use port 'yyyy'
     c) else look for 'sealms' entry in SERVICES file,
     d) else look for 'gui400lic' entry in SERVICES file,
     c) else use default port 1025.

	 
1.2 Installation
There are two installation methods - automatic vs manual.
Automatic installation means that an FTP connection is initiated and 
transferring the files from the PC to the host application begins 
automatically.
Manual installation means that the LegaSuite License and Message Server 
is installed manually to a local PC where it can be transferred to 
the target host application at a later time.
The Setup Wizard will provide instructions for installation.
Additional information is provided in the InstallationGuide PDF in the 
Documentation folder.

If you have any questions or suggestions for enhancements then
please contact your local supplier, Rocket LegaSuite Office, or
Rocket LegaSuite Headquarters directly:

                   Rocket LegaSuite
           http://seagull.rocketsoftware.com/


